
LA-IS6N-F0206

# 2\*100Base-FX, 6\*10/100Base-TX Industrial Ethernet Switch (PoE Optional)

***Highlight Information***

LA-XXX/LAM-XXX Series

For LA-XXX Series

For LA-XXX Series



**Introduction**

This device is 2\* 100Base-FX & 6\*10/100Base-TX Industrial Ethernet Switch. Through the fanless heat dissipation circuit design, wide range of working environment temperature, high protection level and other technologies, it provides excellent industrial quality with high/low temperature resistance and lightning protection, and enhances the reliability and safety of industrial networks.

It can better meet the deployment requirements of rail transit, safe city, intelligent transportation, outdoor monitoring and other harsh environments.

**Features**

**Input Voltage:** DC12~58V **Operating Temperature:** -40℃ ~ +75℃


**Shell:** IP40 protection, fanless design **Test Report:** CCC, RoHS, FCC, CE

**Anti-static:** 8KV-15KV **MTBF:** 100000 Hours

**Specifications**

|  |  |
| --- | --- |
| PART NO | LA-IS6N-F0206 |
| Provider Mode Ports | |
| Fixed Port | 2\*100 Base-FX， 6\*10/100Base-TX |
| Power Interface | Phoenix terminal, redundant dual power supply |
| LED Indicators | PWR，OPT ,NMC，ALM |
| DIP Switch | |
| 1 C/D | Remote PD Reset |
| 2 LGY | Stand/Non-standard PoE Mode |
| 3 VLAN | Port Isolation |
| 4 RST | Reset |
| Cable Type & Transmission Distance | |
| Twisted-pair | 0-100m（CAT5e,CAT6） |
| Monomode Optical Fiber | 20/40/60/80/100KM |
| Multimode Optical Fiber | 550m |
| Network Topology | |
| Ring Topology | Unsupported |
| Star Topology | Support |
| Bus Topology | Support |
| Tree Topology | Support |
| Hybrid Topology | Support |
| Electrical Specifications | |
| Input Voltage | DC12-58V |
| Total Power Consumption | <6W |
| Voltage Alarm | Support |
| Layer 2 Switching | |
| Switching Capacity | 5.6G |
| Packet Forwarding Rate | 4.16Mpps |
| MAC Address Table | 8K |
| VLAN | Unsupported |
| Buffer | 1M |
| Forwarding Delay | <5us |
| MDX/MIDX | Support |
| Flow Control | Support |
| Jumbo Frame | 1632Bytes |
| Watch Dog | Support |
| Port Isolation | Support |
| Environment | |
| Operating Temperature | -40℃~+75℃ |
| Storage Temperature | -40℃~85℃ |
| Relative Humidity | 5%~95% （non-condensing） |
| Thermal Methods | Fanless, natural cooling |
| MTBF | 100,000 hours |
| Mechanical Dimensions | |
| Product Size | 143X104X48mm (W×H×D) |
| Installation Method | DIN-rail |
| Weight | 0.5KG around |
| EMC & Ingress Protection | |
| IP Level | IP40 |
| Surge Protection of Power | IEC 61000-4-5 Level 3 (4KV/2KV）（8/20us) |
| Surge Protection of Ethernet Port | IEC 61000-4-5 Level 3 (4KV/2KV）（10/700us) |
| RS | IEC 61000-4-3 Level 3（10V/m） |
| EFI | IEC 61000-4-4 Level 3（1V/2V） |
| CS | IEC 61000-4-6 Level 3（10V/m） |
| PFMF | IEC 61000-4-8 Level 4（30A/m） |
| DIP | IEC 61000-4-11 Level 3 （10V） |
| ESD | IEC 61000-4-2 Level 4（8K/15K） |
| Free Fall | 0.5m |
| Authentication | |
| Authentication | CCC/CE/FCC/RoHS |

**Dimensions**



Bottom View

Front view Side view Back view Top view

**Ordering Information**

|  |  |
| --- | --- |
| PART NO | DESCRIPTION |
| LA-IS6N-F0206 | 2\*100Mbps SFP Port, 6\*10/100Mbps RJ45 Port |

**Accessories**

|  |  |
| --- | --- |
| PART NO | DESCRIPTION |
| LA-IS6N-F0206 | device, terminals, specification, certificate  adapter(optional) |